Ventilation









Inside temp with specified ventilation













Suppl heat







Freely ventlated























To determine the aperture to achieve a specified V, evaluate V for α= αmin and 1.0.

Evaluate ventilation and temperature hike for minimum and maximum openings.





Check inside temperature at Vopt















